##### SCHEDULE “B”

Scope of work

Joint Sealants.

Clean and prepare surface to receive new sealant and apply backer rod where necessary at the

following locations:

At all exterior windows perimeter where frames meets brick or siding

At all exterior where stone and soffit meets and close all gaps

At exterior main door frame perimeter and balcony doors

At exterior vertical joints between dissimilar materials

Exterior pipe penetrations, vents, light fixtures and electrical outlets

Supply lift equipment and transportation cost

**All material, labour and lift equipment included in pricing.**