|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **DISTRIBUTION:** | Anne Federico | Sam Allegranza | **Surveyor:** | Rady -Pentek | **Windows:** | Brown Windows |
| Julian Baldassarra | Vera Vien | Gina Griffo | **Lumber:** | KOTT | **Kitchen:** | Selba |
| Carlo Baldassarra | Elaine Galley | Alex Micoli | **Carpenter:** | FED | **Railing:** | Airport |
| Armando Baldassarra | Danny Mizzoni | Michael Volpe | **Forming:** | Lee Rocca | **Stone Detail:** | N/A |
| Michael Baglione | Mario Farano |  | **Steel:** | Mansteel | **Roof:** | Chouinard |
| Chris Tozzi | Sandra Aversa |  | **Heating :** | Montwest | **Panels:** | N/A |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **LOT** | **MODEL** | **EL** | **2ND FLR LAYOUT** | **MAIN FLR HEIGHT** | **BAST POUR HIEGHT** | **WALK UP** | **DECK** | **NOTES** |
| 1 | Celestial 2 | 1 | 5 BED | 10’ | 7’ 8” | NO | NO | - Lower level – enlarge basement windows (30” x 24”)-Lower level – add 2 new basement windows (30” x 24”)-Main level – reduce closet in sunken entrance from garage + replace library single door with double doors-Upper level – relocate closet in bed 3 + delete on sink/vanity + replace tub to shower in ens 3-Upper level – delete wall for frameless glass shower in ensuite |
| 2 | Celestial 1 | 2 | Std. | 10’ | 8’ 6” | YES | YES | -Lower level – enlarge basement windows (30” x 24”)-Main level – custom main level plan – see construction summary for sketch-Upper level – custom upper floor layout – see construction summary for sketch. |
| 3 | Amelia 1 | 1 | Std. | 10’ | 7’ 8” | NO | YES | -Standard plan |
| 4 | Amelia 2 | 2 | Std. | 10’ | 7’ 8” | YES | YES | -Lower level – enlarge basement windows (30” x 24”)-Upper level - change tub to shower at shared ensuite -Upper level - delete wall in master ensuite for frameless shower enclosure |
| 5 | Amelia 3 | 2 | Std. | 10’ | 7’ 8” | NO | YES | -Lower level – enlarge basement windows (30” x 24”)-Lower level – add 3 new basement windows (30” x 24”)-Main level – revise living/dining room archways + changes to kitchen layout – see sketch-Upper level – increase hallway width to allow double doors to master bed + delete wall for frameless glass shower in ensuite + replace tubs in ensuite 3 and 4 with showers |
| 6 | Amelia 3 | 1 | 5 BED | 10’ | 7’ 8” | NO | YES | -Lower level – enlarge basement windows (30” x 24”)-Lower level – add 3 new basement windows (30” x 24”)-Main level – relocate window in kitchen + revise living/dining room archways + delete sink from island and install on stove wall + new layout for kitchen-Upper level – delete wall for frameless glass shower in ensuite + replace tubs in ensuite 3 and main with shower |
| 7 | Amelia 2 | 2 | Std. | 10’ | 7’ 8” | YES | NO | -Lower level – enlarge basement windows (30” x 24”) |
| 8 | Amelia 2 | 1 | Std. | 10’ | 7’ 8” | YES | NO | -Lower level – enlarge basement windows (30” x 24”) |
| 9 | Amelia 3 | 2 | 5 BED | 10’ | 7’ 8” | NO | NO | -Lower level – enlarge basement windows (30” x 24”)-Lower level – add 1 new basement window (30” x 24”)-Main level – revise archways at living/dining: to be cambered + add half walls with nib walls and columns + revise kitchen layout-Upper level – reduce closet by 4” in bedroom 2 + replace ensuite 2 and 3 tubs with showers |
| 10 | Celestial 2 | 2 | 5 BED | 10’ | 8’ 6” | YES | YES | -Lower level – enlarge basement windows (30” x 24”)-Upper level – delete wall in master ensuite for frameless shower enclosure-Upper level – change tubs to showers in ensuite 2/3 and ensuite 4 |
| 11 | Liana 2 | 1 | Std. | 9’ | 7’ 8” | YES | YES | -Lower level – enlarge basement windows (30” x 24”) |
| 12 | Celestial 1 | 1 | 5 BED | 10’ | 8’ 6” | YES | YES | -Lower level – enlarge basement windows (30” x 24”)-Main level – close arches to living/dining room + add uppers/base in kitchen + relocate/add French door to library-Upper level – delete wall in master ensuite for frameless shower enclosure + replace ensuite 2/3 tub with shower + add second sink to ensuite 4/5 + delete linen closet and extend master walk in closet |
| 13 | Amelia 12 | 1 | Std. | 10’ | 7’ 8” | YES | YES | -Lower level – enlarge basement windows (30” x 24”)-Lower level – add 1 new basement window (30” x 24”)-Upper level – change tub to shower at ensuite 4  |
| 14 | Amelia 3 | 2 | 5 BED | 10’ | 7’ 8” | YES | YES | -Lower level – enlarge basement windows (30” x 24”)-Lower level – add 2 new basement windows (30” x 24”)-Upper level – replace ensuite 3 tub with shower |
| 15 | Amelia 12 | 2 | Std. | 10’ | 8’6” | YES | YES | -Lower level – enlarge basement windows (30” x 24”)-Lower level – add 1 new basement window (30” x 24”)-Upper level - replace ensuite 2 and shared bath tubs with showers |
| 16 | Liana 3 | 2 | Std. | 9’ | 7’ 8” | YES | NO | -Lower level – enlarge basement windows (30” x 24”)-Upper level – frameless glass shower at master ensuite + replace main bath tub with shower |
| 17 | Liana 2 | 1 | Std. | 9’ | 7’ 8” | NO | NO | -Lower level – enlarge basement windows (30” x 24”)-Lower level – add 1 new basement window (30” x 24’)-Upper level – add ensuite to bedroom 2 + relocate closet in bed 2 + modify walk in closet to accommodate ensuite |
| 18 | Liana 2 | 2 | Std. | 10’ | 8’6” | YES | YES | -Lower level – enlarge basement windows (30” x 24”)-Main level – increase main floor height to 10’-Upper level – add ensuite to bedroom 2 + relocate closet in bed 2 + modify walk in closet to accommodate ensuite |
| 19 | Liana 3 | 2 | Std. | 9’ | 7’ 8” | NO |  NO | -Lower level – enlarge basement windows (30” x 24”)-Upper level – delete door to main bath water closet |
| 20 | Liana 2 | 1 | Std. | 9’ | 7’ 8” | NO | NO | -Standard plan |
| 21 | Indigo 1 | 2 | Std. | 10’ | 7’ 8” | YES | NO | -Lower level – enlarge basement windows (30” x 24”)-Upper level – replace ensuite 4 tub with shower |
| 22 | Liana 2 | 2 | Std. | 9’ | 7’ 8” | YES | YES | -Lower level – enlarge basement windows (30” x 24”) |
| 23 | Liana 3 | 2 | Std. | 9’ | 7’ 8” | NO | NO | -Lower level – enlarge basement windows (30” x 24”)-Main level – Relocate fireplace to side wall + add double doors at front entrance + flip powder room and closet in foyer -Upper level – extend linen closet with double doors + replace free standing tub in ensuite with tub deck |
| 24 | Liana 3 | 1 | Std. | 9’ | 7’ 8” | NO | NO | -Lower level – enlarge basement windows (30” x 24”)-Lower level – complete finished bathroom-Upper level – replace tub in main bath with shower |
| 25 | Liana 2 | 1 | Std. | 9’ | 7’ 8” | YES | NO | -Lower level – enlarge basement windows (30” x 24”) |
| 26 | Belle 1 | 2 | Std. | 10’ | 7’ 8” | YES | NO | -Lower level – enlarge basement windows (30” x 24”)-Lower level – add 2 new basement windows (30” x 24’) |
| 27 | Indigo 1 | 1 | Std. | 10’ | 7’ 8” | NO | NO | -Lower level – enlarge basement windows (30” x 24”)-Upper level – delete wall for frameless glass shower in ensuite + replace tubs in ensuite 2/3 and 4 with showers |
| 28 | Liana 1 | 1 | Std. | 9’ | 7’ 8” | NO | NO | -Lower level – enlarge basement windows (30” x 24”)-Lower level – add 1 new basement window (30” x 24’)-Upper level – revised upper level layout to accommodate added ensuite to bed 2 – see sketch |
| 29 | Liana 1 | 2 | 4 BED | 9’ | 7’ 8” | YES | NO | -Lower level – enlarge basement windows (30” x 24”) |