# ALL PROJECTS

CONTRACT SPECIFICATIONS

# EXTERIOR PARGING

1. Required Application Areas:

The contractor shall apply Parging between masonry and adjacent door and window frames

 or trim. Contractor to apply sand mortar with bonding agent to all exposed foundation. Contractor to properly prep all surfaces to ensure a smooth even finish. Contractor shall parge all front riser steps but keeping the actual step clean. Parging to be applied between April 15 and November 1st (Weather permitting)

1. Preparation: All applied surfaces must be dry and clean, and loose dust must be thoroughly brushed off before parging application
2. Restrictions: (Application Temperature) No work is to be performed at temperatures below freezing unless tarping or heating techniques are applied. .
3. .All materials and labour shall conform to the Ontario Building Code.
4. The Contractor shall report to the Owner’s Site Superintendent any deficiencies of the units, which could affect the quality of their job. The contractor shall also assure that all parging contact areas are free and clear of dust and debris, or any solvents or materials that may adversely affect the bonding of the parging to the substrate to which it is applied. No further work is to be performed to this area until such time as the Site Superintendent has addressed these concerns.
5. The Contractor shall provide to the Owner, prior to starting his work, proof of a two million dollar liability insurance naming the Contractor and the Owner jointly for the duration of the contract.
6. The Contractor shall remove all waste materials generated by his employees and agents from the units to containers as directed by the Site Superintendent. This “clean-up” shall be performed immediately upon request of the Site Superintendent.
7. The Contractor shall take all means necessary to ensure his employees and agents comply with all requirements of the Ontario Health and Safety Act and the Owner’s Safety Policy Statement.
8. The Contractor shall provide, upon demand, to the Owner, a certificate of clearance from Worker’s Compensation.
9. The Contractor shall provide to the Owner a warranty on labour and materials equal to the Owner’s obligations under the Ontario New Home Warranty Program.